Packet Tracer - Connect a Router to a LAN

# Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| R1 | G0/0 | 192.168.10.1 | 255.255.255.0 | N/A |
| R1 | G0/1 | 192.168.11.1 | 255.255.255.0 | N/A |
| R1 | S0/0/0 (DCE) | 209.165.200.225 | 255.255.255.252 | N/A |
| R2 | G0/0 | 10.1.1.1 | 255.255.255.0 | N/A |
| R2 | G0/1 | 10.1.2.1 | 255.255.255.0 | N/A |
| R2 | S0/0/0 | 209.165.200.226 | 255.255.255.252 | N/A |
| PC1 | NIC | 192.168.10.10 | 255.255.255.0 | 192.168.10.1 |
| PC2 | NIC | 192.168.11.10 | 255.255.255.0 | 192.168.11.1 |
| PC3 | NIC | 10.1.1.10 | 255.255.255.0 | 10.1.1.1 |
| PC4 | NIC | 10.1.2.10 | 255.255.255.0 | 10.1.2.1 |

# Objectives

Part 1: Display Router Information

Part 2: Configure Router Interfaces

Part 3: Verify the Configuration

# Background

In this activity, you will use various **show** commands to display the current state of the router. You will then use the Addressing Table to configure router Ethernet interfaces. Finally, you will use commands to verify and test your configurations.

**Note**: The routers in this activity are partially configured. Some of the configurations are not covered in this course but they are provided to assist you in using verification commands.

## Display Router Information

### Display interface information on R1.

**Note**: Click a device and then click the **CLI** tab to access the command line directly. The console password is **cisco**. The privileged EXEC password is **class**.

#### Questions:

* + 1. Which command displays the statistics for all interfaces configured on a router?

***show interfaces***

* + 1. Which command displays the information about the Serial 0/0/0 interface only?

show interface Serial0/0/0

* + 1. Enter the command to display the statistics for the Serial 0/0/0 interface on R1 and answer the following questions:
       1. What is the IP address configured on **R1**?

209.165.200.225/30

* + - 1. What is the bandwidth on the Serial 0/0/0 interface?

1544 Kbit

* + 1. Enter the command to display the statistics for the GigabitEthernet 0/0 interface and answer the following questions:
       1. What is the IP address on **R1**?

None configuredType your answers here.

* + - 1. What is the MAC address of the GigabitEthernet 0/0 interface?

000d.bd6c.7d01 Type your answers.

* + - 1. What is the bandwidth (BW) of the GigabitEthernet 0/0 interface?

1000000 Kbit Type your answers here.

### Display a summary list of the interfaces on R1.

#### Questions:

* + 1. Which command displays a brief summary of the current interfaces, interface status, and the IP addresses assigned to them?

show ip interface briefType your answers here.

* + 1. Enter the command on each router and answer the following questions:
       1. How many serial interfaces are there on **R1** and **R2**?

R1: 2, R2: 2Type your answers here.

* + - 1. How many Ethernet interfaces are there on **R1** and **R2**?

R1: 6, R2: 2Type your answers here.

* + - 1. Are all the Ethernet interfaces on **R1** the same? If no, explain the difference(s).

***No, there are 2 gigabit ethernet interfaces and 4 fast ethernet interfaces. Gigabit supports speeds of 1000 Mbit/s and fast ethernet supports up to 100 Mbit/s***

### Display the routing table on R1.

#### Questions:

* + 1. What command displays the contents of the routing table?

show ip routeType your answers here.

* + 1. Enter the command on **R1** and answer the following questions:
       1. How many connected routes are there (uses the **C** code)?

1Type your answers here.

* + - 1. Which route is listed?

209.165.200.224/30 Type your answers here.

* + - 1. How does a router handle a packet destined for a network that is not listed in the routing table?

***If a default path or gateway of last resort is not set, then the router will drop a packet that is destined for a network not listed in the routing table.***

## Configure Router Interfaces

### Configure the GigabitEthernet 0/0 interface on R1.

* + 1. Enter the following commands to address and activate the GigabitEthernet 0/0 interface on **R1**:

Open configuration window

R1(config)# **interface gigabitethernet 0/0**

R1(config-if)# **ip address 192.168.10.1 255.255.255.0**

R1(config-if)# **no shutdown**

%LINK-5-CHANGED: Interface GigabitEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0, changed state to up

* + 1. It is good practice to configure a description for each interface to help document the network. Configure an interface description that indicates the device to which it is connected.

R1(config-if)# **description LAN connection to S1**

* + 1. **R1** should now be able to ping PC1.

R1(config-if)# **end**

%SYS-5-CONFIG\_I: Configured from console by console

R1# **ping 192.168.10.10**

Type escape sequence to abort.

Sending 5, 100-byte ICMP Echos to 192.168.10.10, timeout is 2 seconds:

.!!!!

Success rate is 80 percent (4/5), round-trip min/avg/max = 0/2/8 ms

### Configure the remaining Gigabit Ethernet Interfaces on R1 and R2.

* + 1. Use the information in the Addressing Table to finish the interface configurations for **R1** and **R2**. For each interface, do the following:
       1. Enter the IP address and activate the interface.
       2. Configure an appropriate description.
    2. Verify interface configurations.

### Back up the configurations to NVRAM.

#### Question:

Save the configuration files on both routers to NVRAM. What command did you use?

copy run startType your answers here.

Close configuration window

## Verify the Configuration

### Use verification commands to check your interface configurations.

* + 1. Use the **show ip interface brief** command on both **R1** and **R2** to quickly verify that the interfaces are configured with the correct IP address and are active.

#### Questions:

How many interfaces on **R1** and **R2** are configured with IP addresses and in the “up” and “up” state?

3Type your answers here.

What part of the interface configuration is NOT displayed in the command output?

Subnet maskType your answers here.

What commands can you use to verify this part of the configuration?

show interfacesType your answers here.

* + 1. Use the **show ip route** command on both **R1** and **R2** to view the current routing tables and answer the following questions:

#### Questions:

* + - 1. How many connected routes (uses the **C** code) do you see on each router?

R1: 3, R2: 3Type your answers here.

* + - 1. How many OSPF routes (uses the **O** code) do you see on each router?

R1: 2, R2: 2Type your answers here.

* + - 1. If the router knows all the routes in the network, then the number of connected routes and dynamically learned routes (OSPF) should equal the total number of LANs and WANs. How many LANs and WANs are in the topology?

5Type your answers here.

* + - 1. Does this number match the number of C and O routes shown in the routing table?

Yes

**Note**: If your answer is “no”, then you are missing a required configuration. Review the steps in Part 2.

### Test end-to-end connectivity across the network.

You should now be able to ping from any PC to any other PC on the network. In addition, you should be able to ping the active interfaces on the routers. For example, the following tests should be successful:

* From the command line on PC1, ping PC4.
* From the command line on R2, ping PC2.

**Note**: For simplicity in this activity, the switches are not configured. You will not be able to ping them.

End of document